{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["中文参数","specification"],"read":"whole","date_system":"1900"}

{"sheet":"中文参数","index":0,"n_rows":48,"n_cols":5,"rows_kept":48,"merged":[[1,0,3,1],[1,2,3,6],[5,0,5,3],[5,4,5,6],[6,0,6,3],[6,4,6,6],[7,0,7,3],[7,4,7,6],[8,0,10,0],[8,1,8,3],[8,4,8,6],[9,1,9,3],[9,4,9,6],[10,1,10,3],[10,4,10,6],[11,0,11,3],[11,4,11,6],[12,0,21,0],[12,1,12,3],[12,4,12,6],[13,1,13,3],[13,4,13,6],[14,1,14,3],[14,4,14,6],[15,1,15,3],[15,4,15,6],[16,1,16,3],[16,4,16,6],[17,1,17,3],[17,4,17,6],[18,1,18,3],[18,4,18,6],[19,1,19,3],[19,4,19,6],[20,1,21,1],[20,2,20,3],[20,4,20,6],[21,2,21,3],[21,4,21,6],[22,0,22,3],[22,4,22,6],[23,0,33,0],[23,1,28,1],[23,2,24,2],[23,4,23,6],[24,4,24,6],[25,4,25,6],[26,4,26,6],[27,4,27,6],[28,4,28,6],[29,1,29,3],[29,4,29,6],[30,1,30,3],[30,4,30,6],[31,1,31,3],[31,4,31,6],[32,1,32,3],[32,4,32,6],[33,1,33,3],[33,4,33,6],[34,0,41,0],[34,1,34,3],[34,4,34,6],[35,1,35,3],[35,4,35,6],[36,1,36,3],[36,4,36,6],[37,1,37,3],[37,4,37,6],[38,1,38,3],[38,4,38,6],[39,1,40,1],[39,2,39,3],[39,4,39,6],[40,2,40,3],[40,4,40,6],[41,1,41,3],[41,4,41,6],[42,0,44,0],[42,1,42,3],[42,4,42,6],[43,1,43,3],[43,4,43,6],[44,1,44,3],[44,4,44,6],[45,0,45,3],[45,4,45,6],[46,0,46,3],[46,4,46,6],[47,0,47,3],[47,4,47,6]]}
[]
["2ZG-6D",null,"高速乘坐式插秧机"]
[]
[]
[]
["产品型号",{"$nulls":3},"2ZG-6D"]
["结构型式",{"$nulls":3},"乘座式"]
["驱动型式",{"$nulls":3},"四轮驱动"]
["外形尺寸","长度（mm）",null,null,3090]
[null,"宽度（mm）",null,null,2220]
[null,"高度（mm）",null,null,2580]
["结构质量（kg）",{"$nulls":3},820]
["配套发动机","型号（中国第三阶段）",null,null,"3TNM72"]
[null,"结构型式",null,null,"立式水冷3 缸柴油机"]
[null,"总排气量（L）",null,null,0.904]
[null,"标定功率（kW）",null,null,18.5]
[null,"标定转速（r/min）",null,null,3600]
[null,"燃油",null,null,"优质柴油"]
[null,"燃油箱容量（L）",null,null,34]
[null,"起动方式",null,null,"电起动"]
[null,"蓄电池","额定电压（V）",null,12]
[null,null,"额定容量（Ah）",null,45]
["单位作业量燃油消耗量(kg/hm )",{"$nulls":3},"2.2～5.6"]
["行驶部","行走轮","结构型式","前轮","防爆轮胎"]
[{"$nulls":3},"后轮","粗轮毂橡胶轮胎"]
[null,null,"直径×宽","前轮","φ650×95"]
[null,null,"（mm）","后轮","φ950×50"]
[null,null,"轮距","前轮",1200]
[null,null,"（mm）","后轮",1200]
[null,"转向方式",null,null,"整体液压转向"]
[null,"变速方式",null,null,"液压式变速（HST）"]
[null,"变速级数（级）",null,null,"主变速：前进后退无级变速（副变速：2挡；防陷变速：2挡）"]
[null,"作业速度（km/h）",null,null,"0～5.94"]
[null,"最小离地间隙（mm）",null,null,500]
["插秧部","插植机构型式",null,null,"旋转式强制插秧"]
[null,"工作行数（行）",null,null,6]
[null,"行距（mm）",null,null,300]
[null,"穴距（mm）",null,null,"100、120、140、160、180、210、240"]
[null,"插秧深度（mm）",null,null,"10～55（7级）"]
[null,"1穴苗数调节量","横向移动次数",null,"20、18、16、14"]
[null,null,"纵向取秧深度（mm）",null,"8～18"]
[null,"平衡机构型式",null,null,"机械式"]
["秧苗条件","秧苗种类",null,null,"块状秧苗"]
[null,"苗高（mm）",null,null,"80～250"]
[null,"叶龄（叶）",null,null,"2.0～4.5"]
["秧盘架（个）",{"$nulls":3},6]
["警报装置",{"$nulls":3},"充电、油压、后退时、水温、秧苗用尽"]
["作业小时生产率（hm²/h）\n                          (亩/h)",{"$nulls":3},"0.2～0.6"]

{"sheet":"specification","index":1,"n_rows":48,"n_cols":5,"rows_kept":48,"merged":[[1,0,3,1],[1,2,3,4],[5,0,5,3],[6,0,6,3],[7,0,7,3],[8,0,10,0],[8,1,8,3],[9,1,9,3],[10,1,10,3],[11,0,11,3],[12,0,21,0],[12,1,12,3],[13,1,13,3],[14,1,14,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[18,1,18,3],[19,1,19,3],[20,1,21,1],[20,2,20,3],[21,2,21,3],[22,0,22,3],[23,0,33,0],[23,1,28,1],[23,2,24,2],[25,2,26,2],[27,2,28,2],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,1,32,3],[33,1,33,3],[34,0,41,0],[34,1,34,3],[35,1,35,3],[36,1,36,3],[37,1,37,3],[38,1,38,3],[39,1,40,1],[39,2,39,3],[40,2,40,3],[41,1,41,3],[42,0,44,0],[42,1,42,3],[43,1,43,3],[44,1,44,3],[45,0,45,3],[46,0,46,3],[47,0,47,3]]}
[]
["2ZG-6D",null,"HIGH SPEED-RIDING TYPE RICE TRANSPLANTER"]
[]
[]
[]
["Model",{"$nulls":3},"2ZG-6D"]
["Structural Type",{"$nulls":3},"Riding Type"]
["Driving Type",{"$nulls":3},"Four-Wheel Drive"]
["Dimension","Length（mm）",null,null,3090]
[null,"Width（mm）",null,null,2220]
[null,"Height（mm）",null,null,2580]
["Weight（kg）",{"$nulls":3},820]
["Engine","Model（Phase III Of China）",null,null,"3TNM72"]
[null,"Structural Type",null,null,"Vertical Type,Water-Cooliong,3 Cylinders Diesel Engine"]
[null,"Displacement（L）",null,null,0.904]
[null,"Rated Power（kW）",null,null,18.5]
[null,"Rated Rotate Speed（r/min）",null,null,3600]
[null,"Fuel Oil",null,null,"High Quality Diesel"]
[null,"Fuel Tank Capacity（L）",null,null,34]
[null,"Start-Up Mode",null,null,"Electric Starter"]
[null,"Battery","Rated Voltage（V）",null,12]
[null,null,"Rated Capacity（Ah）",null,45]
["Fuel Consumption(kg/hm )",{"$nulls":3},"2.2～5.6"]
["Driving","Driving Wheel","Structural Type","Front","Anti-Explosion Tire"]
[{"$nulls":3},"Rear","Thick Hub Rubber Tire"]
[null,null,"Diameter×Width (mm)","Front","φ650×95"]
[{"$nulls":3},"Rear","φ950×50"]
[null,null,"WheelBase (mm)","Front",1200]
[{"$nulls":3},"Rear",1200]
[null,"Steering Mode",null,null,"Integral Hydraulic Steering"]
[null,"Gearshift Type",null,null,"Hydraulic Transmission（HST）"]
[null,"Number Of Transmission Gear（Stage）",null,null,"Main Transmission:CVT Of Forward And Backward（Auxiliary Transmission:2 Stages;Anti-Stuck Transmission:2 Stages）"]
[null,"Working Speed（km/h）",null,null,"0～5.94"]
[null,"Minimum Ground Clearance（mm）",null,null,500]
["Transplanting","Transplanter Type",null,null,"Rotary Forced Transplanting"]
[null,"Rows Number（Rows）",null,null,6]
[null,"Row Spacing（mm）",null,null,300]
[null,"Hill Spacing（mm）",null,null,"100、120、140、160、180、210、240"]
[null,"Transplanting Depth（mm）",null,null,"10～55（7 Gears）"]
[null,"Adjustment Number Of 1 Seeding","Number Of Lateral Movenments",null,"20、18、16、14"]
[null,null,"Vertical Seeding Depth（mm）",null,"8～18"]
[null,"Balance Mechanism Type",null,null,"Mechanical"]
["Seeding Requirement","Type Of Seeding",null,null,"Lump Seeding"]
[null,"Height Of Seeding（mm）",null,null,"80～250"]
[null,"Leaf Age（Leaf）",null,null,"2.0～4.5"]
["Seeding Tray（PCS）",{"$nulls":3},6]
["Alarming Device",{"$nulls":3},"Charging、Fuel Pressure、Reverse、Water Temperature、Seeding Exhaustion"]
["Productivity（hm²/h）\n                          (亩/h)",{"$nulls":3},"0.2～0.6"]